IFCONFIG( 8) Eighth Edition IFCONFIG (8)

NAME

ifconfig - configure a TCP/IP device

SYNOPSISS

ifconfig [- I ip-device] [- h ipaddr] [- n netmask] [-iv]

DESCRIPPTION Ifconfig initializes a TCP/IP device setting the IP address and/or netmask. It will report the address and netmask set. This command may be used if the system has not been configured properly yet. It is only used at boot time to set a fixed address for a system without a physical ethernet. Normally the inet task will find it out by itself from the RARP server.

OPTIONS

- h The decimal TCP/IPaddress to set.

- n The netmask to set.

- i Don’t set the IP address or netmask if already set. This way ifconfig cannot interfere if the numbers have been found out by RARP.

- v Report IP address and netmask. This is thedefault action if there areno other options.

SEE AALSO

hostaddr (1),rarpd (8),netdefault (8), boot(8).

AUTHOR

Kees J. Bot (kjb@cs.vu.nl)

Page 1 September 3, 1999