REPARTITION (8) Eighth Edition REPARTITION (8)

NAME

repartition - load a partition table

SYNOPSISS

repartition device [partition-file]

DESCRIPPTION Repartition uploads a new partition table for the partitions of device. The table is obtained from the first sector of partition-file if given, deviceotherwise. Devicemay refer to the whole drive or a primary partition, depending on whether you want to upload a partition or a subpartition table. The partitions will be truncated to fit within the enclosing device like the disk driver does, unless the numbers are coming from partition-file.

EXAMPLES

repartition /dev/hd0 repartition /dev/hd4 /etc/hd4.table

Reload the partition table of drive 0 setting /dev/hd[1- 4], and the subpartition table of /dev/hd4 setting /dev/hd4[a- d] using a file. The latter may be useful if you need more than the 4 subpartitions a single Minix partition gives you.

DIAGNOSTICCS The new table is printed on standard output.

FILLES

/dev/hd[0-9]

SEE AALSO

hd(4), part (8).

BUGS

The disk must be in use for the changes to stick. The partition table of an idle disk will be reloaded on the first open.

AUTHOR

Kees J. Bot (kjb@cs.vu.nl)

Page 1 September 3, 1999