PS(1) Eighth Edition PS(1)

NAME

ps - process status SYNOPSISS

ps [-alxU] [kernel mm fs] OPTIONS

- a Print all processes with controlling terminals - l Give long listing - x Include processes without a terminal EXAMPLES ps - axl # Print allprocesses and tasks in long format DESCRIPPTION Ps prints the status of active processes. Normally only the caller’s own processes are listed in short format (the PID, TTY, TIME and CMD fields as explained below). The long listing contains: F Kernel flags: 001: free slot 002: no memory map 004: sending; 010: receiving 020: inform on pending signals 040: pending signals 100: being traced. S State: R: runnable W: waiting (on a message) S: sleeping (i.e.,suspended on MM or FS) Z: zombie T: stopped UID, PID, PPID, PGRP The user, process, parent process and process group ID’s. SZ Size of the process in kilobytes.

RECV Process/task on which a receiving process is waiting or sleeping. TTY Controlling tty for the process.

TIME Process’ cumulative (user + system) execution time. CMD Command line arguments of the process. The files /dev/{mem,kmem}are used to read the system tables and command line arguments from. Terminal names in /dev are used to generate the mnemonicnames in the TTY column, so ps is independent of terminal naming conventions.

Page 1 September 3, 1999